This file contains installation instructions for the included Intel 82371FB
and  82371SB  PIIX Bus Master IDE Drivers.  The driver versions included in
this release are:
   Windows 95 Driver - Version 2.64
   Windows NT Driver - Version 1.68
   IBM OS/2 Driver   - Version 2.06
===========================================================================
INSTALLATION PROCEDURES
----------------------------------------------------------------------------
1.  Create a directory on your hard drive for the appropriate file for your
    operating system:
      For Windows 95  - bmide_95.exe
      For Windows NT  - bmide_nt.exe
      For IBM OS/2    - bmideos2.exe

2.  Copy the appropriate file to the newly created directory.

3.  Run the self-extracting file to expand the program files.

4.  Driver Installation for Windows 95:
    Run the setup program included with the files that was extracted above
    by clicking on SETUP.EXE from Windows "File Manager" or "Explorer."
    NOTE:  Also see auto install procedures. If using OEM Version of Win 95
    CD-ROM on PIIX3 based systems see also " 82371SB PIIX3 Application Note
    #3 Microsoft Window Support for PIIX3 IDE Controller".

4b. Driver Installation for IBM OS/2 and Windows NT3.51/4.0:
    Run  SETUP.EXE  and  follow the installation instructions in README.TXT
    file which is extracted to the driver installation directory.


BMREADME.TXT 10/7/96
